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Product/Service Purchased                                                Quality Code
	Hardware/Products
	QC01, QC02, QC05, QC06, QC09, QC13, QC15, QC16, QC17, QC21, QC22, QC23, QC24, QC25, QC26, QC27

	Outside Processing
	QC01, QC02, QC03, QC05, QC06, QC10, QC11, QC13, QC14, QC15, QC17, QC21, QC22, QC24, QC25, QC26, QC27

	Outside Service/Calibration
	QC01, QC02, QC05, QC06, QC07, QC08, QC09, QC10, QC12, QC13, QC14, QC15, QC16, QC17, QC19, QC21, QC22, QC24, QC25, QC26, QC27

	Quality Code
	Title
	Requirement

	QC01
	Quality System
	Supplier shall establish and maintain a Quality System acceptable to RCV Interconnect, Inc., for the goods and/or services purchased under this purchase order. 

	QC02
	AS9100 Compliant
	The supplier is required to maintain a Quality System in compliance to AS9100.  If facility is not certified to AS9100, RCV Interconnect, Inc. reserves the right to conduct surveillance at supplier's facility to make final determination that Supplier's Quality System meets the requirements, and/or supplier will be required to complete a Supplier Survey Questionnaire. 

	QC03
	NADCAP Approval
	Special processing NADCAP approval is required. The special process requirements will be listed on the actual purchase order.

	QC04
	Supplier Furnished Material
	Supplier shall submit Chemical and Physical test reports in accordance with the latest material specifications and revision. Distributors must provide a certification verifying the materials traceability to the Mill test reports when supplied.

	QC05 
	Sub-Contractor Flow Down
	Supplier is required to flow down the requirements of this purchase order, including terms and conditions, to the Supplier's subcontractors. Flow down of key characteristics is required when specified on the face of purchase order. Supplier is to notify RCV Interconnect, Inc. of changes in product and/or process, changes of suppliers, changes of manufacturing facility location, and obtain organization approval within 1 business day.

	QC06
	Record Retention and Disposition
	As a minimum, the Supplier is to retain records for at least 7 years from the date of shipment under each applicable order for all products/part numbers unless otherwise specified in the order.  In special circumstances, the purchase order will identify the actual required number of years that the records should be maintained. After the minimum retention period is achieved, suppliers may disposition the records as archive or destroy at their discretion.

	QC07
	Calibration
	The Supplier's equipment shall be calibrated in accordance to NIST standard (ISO 17025/ISO 10012-1/ANSI Z540-1) traceable to national or international measurement standards.

	QC08
	RCV Interconnect, Inc. Furnished Property
	Supplier is to return all furnished property to RCV Interconnect, Inc. at the completion of the purchase order. Furnished property may include but is not limited to the following: drawings, process specification, tooling, fixtures, and excess material.

	QC09
	Parts Identification
	The Supplier is to identify parts in accordance with purchase order requirements.

	QC10
	Nonconformance/Corrective Action
	The Supplier is to notify RCV Interconnect, Inc. of a Nonconformance prior to shipping parts. In addition, the Supplier will maintain a system of handling non-conformances and corrective actions.

	QC11
	Special Processing Approval
	If the Supplier is to perform a special process, (Special processing may include, but is not limited to, the following processes: heat-treating, stress relieving or Nondestructive testing), RCV Interconnect, Inc. shall identify the specific process specification on the purchase order. If the Supplier is not currently approved for the specified process, it is the Supplier's responsibility to notify RCV Interconnect, Inc. immediately.

	QC12
	Dimensional Inspection Report
	The Supplier is to document an actual dimensional inspection report, when required by RCV Interconnect, Inc., and submit it with shipment.

	QC13
	First Article Inspection
	The Supplier is to submit a First Article, per AS9102B, when required by RCV Interconnect, Inc. It will identify all of the process specifications and dimensional data associated per applicable standards and/or drawings.

	
QC14
	Measuring & 
Test Equipment
	All measuring and test equipment shall be calibrated in accordance with industry and process specification standards.

	QC15
	Packaging Protection
	Supplier will package parts in a manner that will protect parts from any kind of damage. No metal to metal contact is ever allowed. The purchase order may specify the manner the parts are to be packaged.

	QC16
	Traceability 
	Supplier is to maintain traceability throughout all stages of production and post-delivery support.

	QC17
	Certificate of Conformance
	A Certificate of Conformance (C of C) is required. The C of C  will state that all of the products or services meet the contractual or purchase order requirements. 

	QC18
	The Boeing Company Approved Process
	The Supplier shall maintain a special process approval from The Boeing Company on this purchase order.

	QC19
	Key Characteristics Data Required
	This purchase order deals with the drawing that identifies key characteristics. Both the Supplier and RCV Interconnect, Inc. should have established a control plan prior to the placement of this purchase order.

	QC20
	BUY AMERICA ACT
	Items procured under this purchase order must be compliant with DFAR 252.225-7000


	QC21
	Right of Entry
	RCV Interconnect, Inc., our customers, and/or any applicable regulatory authority reserve the right to access the supplier’s facilities, at any level of the supply chain, involved in the order and to all applicable records. Reason for access may include inspection of the item on order, status of the item, or reviewing quality records pertaining to the purchase order in question.

	QC22
	QMS Awareness
	Suppliers Personnel must be made aware of:
•	their contribution to product or service conformity;
•	their contribution to product safety;
•	the importance of ethical behavior.

	QC23
	Counterfeit Prevention
	Suppliers must have a process in place to prevent the use of counterfeit parts/materials.

	QC24
	Control & Monitoring Requirements
	Suppliers must maintain a Quality Level ≥95% and an OTD level ≥95%. If levels drop below target, supplier will be notified and may be placed on conditional status or disapproved if not corrected.

	QC25
	FOD
	Suppliers shall ensure that Foreign Object Debris/Damage (FOD) if any, is removed before the shipment. Wherever applicable, supplier will flow down this requirement to its sub-tier suppliers.

	QC26
	ITAR
	The data attached/enclosed may contain information (including technology and technical data) which is subject to the U.S. International Traffic in Arms Regulations (ITAR) or Export Administration Regulations (EAR). This information may not be exported, released, or disclosed to foreign persons either inside or outside the United States without first obtaining the proper U.S. export license or written authorization. In addition, the information and articles described herein are either patented or proprietary, and the copying or reproduction thereof is prohibited without RCV Interconnect, Inc. prior written consent.

	QC27
	Shipping Terms 
	Unless otherwise provided in the Purchase Order, delivery is F.O.B. the destination location stated in the Purchase Order. At any time during the duration of the Order, RCV Interconnect, Inc. reserves the right to change the F.O.B. shipping destination or method to any location within the continental United States designated by RCV Interconnect, Inc.. Supplier will be notified of this change via E-Mail. Supplier must provide acknowledgement of change via E-Mail within 1 business day. 



T&C Procurement		Page 2 of 2 

image1.png
NNNNNNNNNNNN




